Core 64 Assembly Instructions

For Dual Board hardware version v0.3

2020-05-21 Draft Version 1

Inventory

Two major component kits are brought together to make one complete Core 64 Badge:

1. Core PCB Frame Assembly
2. Logic PCB and everything else

|  |  |  |  |
| --- | --- | --- | --- |
| Item No. | Description | Qty | Core 64 P/N |
| 1 | Core 64 Frame Board (PCB 85x85mm) with all SMD components pre-assembled | 1 pc |  |
| 2 | Magnet wire (16x100mm + 750mm) | 2350 mm (92 in.) |  |
| 3 | Cores | 68 pcs |  |
| 4 | Header Pins 1 row x 16 pin 0.1” SMD or TO | 2 pcs |  |
| 5 |  |  |  |
|  | Solder, flux, and other tools are not included |  |  |

Tools Required

Ruler, wire cutter, forceps (tweezers or small needle nose pliers), soldering pencil, small gauge solder, flux pen, isopropyl alcohol, q-tips, kim wipes, flux remover, multimeter,

Optional: magnifier, circuit board holder,

Preparation

Clean all of the wire with IPA and a soft lint free wipe. This ensures there are no sticky spots or bits of fuzz that will make threading and weaving difficult. It’s a delicate process and you don’t want to tug hard to overcome sticky spots.

Cut 16 pcs of magnet wire, each 100 mm long. These are the grid wires.

Set aside the long uncut piece to be used as the sense wire later.

Assembly Procedure

Horizontal Grid Wires

For each grid wire, using your fingers, bend one end, at 1 cm long, at a right angle to the other 9 cm of wire. A soft bend is preferred instead of a sharp bend which can lead to the wire breaking off. This allows the board to be held up-side-down and the wires won’t fall out during solder. This also provides a length of wire to pull on during the last step of assembly, which is to straighten and tighten all of the grid wires. Don’t cut the extra wire off until all assembly is complete!

Place the Core 64 Frame Board up-side-down in a PCB work holder. The components will be facing up.

Insert the long end of the bent grid wire in hole YL0. The long end of the wire hangs straight down from the top face of the board for now, which is facing down.

The YL0 to 7 wires are all round solder pads. Skip the square sense wire solder pads for now. Those will be used after the 8x8 grid wires and cores are assembled.

Repeat this step for all YL# wires.

Solder the YL0 to 7 grid wires from the backside. Use flux and enough heat to ensure a good electrical connection is made and the burnt enamel on the magnet wire is displaced out of the solder joint. Plan to dwell with the solder pencil at the join for 5 seconds to ensure the enamel is burned away. We will verify the continuity later, and we will be reheating the some of the joints to tighten the grid of wires later.

Flip the board over so the top is up and the long ends of the grid wires are standing up. Clean any fuzz off the wires by gently pinching at the bottom of the wire and sliding your fingers up. You could also use IPA and q-tip to make sure there is no tape residue. This makes it easier to slide the cores on.

Sort the cores in groups of 8. I suggest two small groups of 4 to make the groups of 8. Carefully thread 8 cores onto each wire that is standing up. After each wire has 8 cores, carefully bend it over at the solder joint to head toward the YR0-7 holes. Count the cores on each wire to make sure there are 8 on each wire. Then insert the free end of the grid wire into the corresponding YR0-7 holes.

Admire your abacus.

Count the cores again. Make sure there are 8 on each wire, suspended in the middle and not caught under the wire near the first solder joint. It’s going to become difficult to back track from here forward. Take a break.

Flip the board over so you can solder on the back side again. Count ‘em again.

On the soldered end of the wire, push the wire down to be flush with the top of the board to prevent any cores from being able to slide on the wire and get caught between the top of the board and the wire.

Solder all 8 of the remaining wire ends. The initial soldering for all 8 can be “close enough.” Then go back and apply gentle tension with your fingers to pull the wire taught while reheating the solder joints to ensure a good connection. Continue to hold the wire 5 seconds after you remove the soldering pencil to avoid cold joints.

This is a good time to make grid wires look straight and tight (but not too tight or the wire will break). Aim for about 70% good enough because you will probably want to re-tighten them after the rest of the threading is completed. It is difficult to maintain tension during the rest of the process because the wire is so soft and if you bump it the tiniest bit, it’ll be deformed. That why the final tightening step is at the very end, just before cutting the excess grid wire.

Continuity check. From the solder joint at each end of each of the grid wires.

Vertical Grid Wires

Now is where it starts to get interesting. We’re going to thread each vertical wire through 8 cores, with the cores in a specific pattern.