|  |  |
| --- | --- |
| Logo  Description automatically generated **CORE BOARD KIT V0.5**  [ ] Qty 1, CORE BOARD PCBA  [ ] Qty 68, Ferrite Cores  [ ] Qty 1, 32AWG enamel wire, 100” long  [ ] Qty 4, Plastic Press Rivet  [ ] Qty 2, Screen Protector Sheet  [ ] Qty 1, 1x40 pin TH 0.1” male header, tall, cuttable  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height | Logo  Description automatically generated **LED MATRIX KIT V0.1 or V0.2**  [ ] Qty 1, LED MATRIX PCBA  [ ] Qty 1, 1x8 pin TH 0.1” male headers, >12mm lg  [ ] Qty 1, Battery Pack  [ ] Qty 1, Foam Tape  [ ] Qty 4, “AAA” Batteries  [ ] Qty 1, Diffuser |
| Logo  Description automatically generated **LOGIC BOARD KIT V0.5**  [ ] Qty 1, LOGIC BOARD PCBA  [ ] Qty 1, 2x3 SAO SOCKET  [ ] Qty 1, STYLUS  [ ] Qty 2, Spherical Magnets, 2.5mm dia. | Logo  Description automatically generated **TEENSY 3.2 KIT V0.5**  ***\*\*\* USER MUST CUT VIN-VUSB \*\*\****  ***\*\*\* ON BOTTOM OF TEENSY \*\*\****  [ ] Qty 1, TEENSY 3.2  [ ] Qty 1, Teensy pinout card  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height, cuttable  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height |
|  |  |
|  |  |
|  |  |