|  |  |
| --- | --- |
| **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** | **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** |
| **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** | **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** |
| **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** | **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** |
| **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** | **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** |
| **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** | **Logo  Description automatically generatedTEENSY 3.2 KIT**  140-000 CORE64-T32-KIT V0.5  [ ] Qty 1, Teensy 3.2 [ ] Pinout card [ ] Programmed  [ ] Qty 1, 2x7 pin SMD 0.1” male header, std. height  [ ] Qty 1, 1x40 pin TH 0.1” male header, std. height  [ ] Qty 2, 1x40 pin TH 0.1” female header, std. height  [ ] Qty 1, Micro USB Cable  **\*\*\* USER MUST CUT VIN-VUSB \*\*\***  **\*\*\* ON BACK SIDE OF TEENSY \*\*\*** |